T1

The T1 is a new platform based on a server that can have up to 9 Blades fitted. Each blade contains two separate servers. The T1 main differentiator (at launch) is that it is the first platform that can take advantage of the QSV (Quick Sync Video) feature of the Intel Processor.

Manual	LInk	Notes
SLP	eri-05-00296-01-00-slp-t1_2064-r00.pdf	System Loading Procedure. READ THIS FIRST!
MPI	env-05-00297-01-00-mpi-t1-2000-r02.pdf	Installation Instruction (MPI) Procedure
FLP	env-05-00298-01-00-flp-t1-2ru-usb-r09.pdf	Firmware loading procedure - USB
SSP	env-05-00299-01-00-ssp-t1-2ru-r05.pdf	SOFTWARE SETUP PROCEDURE
FBP	Configuration Guide