{ "chassis": { "serialNumber": "2TNWPK4", "partNumber": "", "productName": "" }, "option_card_slots": [ { "vendorDeviceId": "0x8086:0x1521", "description": "PCIe 4x Port 1G NIC", "marketingCode": "MKP/HWO/PCI/NIC/1G/4PORT", "partNumber": "S16849", "thirdPartyPartNumber": "PCIE-2131NP-00A1E", "deviceName": "Dell 4x 1G NIC", "slotNumber": 1, "pciBusAddress": "0000:81:00.0" }, { "vendorDeviceId": "0x1a0e:0x0882", "description": "PCIe 8 SDI - 2x12G 6x3G SDI/ASI I/O", "marketingCode": "MKP/HWO/PCI/SDI/8", "partNumber": "S16977", "thirdPartyPartNumber": "DTA-2178", "deviceName": "Dektec 2178 SDI/ASI", "slotNumber": 5, "pciBusAddress": "0001:01:00.0" }, { "vendorDeviceId": "0x15b3:0x101d", "description": "PCIe 2 Port 25G NIC supporting ST 2110 and 2022-7", "marketingCode": "MKP/HWO/PCI/NIC/25G/2PORT/B", "partNumber": "S17080", "thirdPartyPartNumber": "MCX621102AN-ADAT", "deviceName": "Mellanox ConnectX-6 Dx", "slotNumber": 6, "pciBusAddress": "0001:41:00.0" } ], "candy": { "present": false, "slotNumber": null }, "dektec": { "DTAPI link version": "6.11.0.240", "devices": "10", "dektec": [ { "type": "2178", "subtype": "0", "pci": "1:0", "fw variant": "1", "fw version": "3", "fw package": "3", "s/n": "2178011812", "slotNumber": 5 } ], "pci cards": "1", "status": "ok" }, "deltacast": { "cards": [], "pci cards": 0, "slotNumbers": [] }, "satellite": { "present": false, "device_name": null, "rfInputCount": 0, "demodCount": 0, "slotNumbers": [], "demodulators": [] }, "cam": { "present": false, "slot_count": 0, "slotNumbers": [], "cams": [] }, "firewall": { "running": true, "zones": { "data": [ "eno16495", "eno16505", "eno16595", "eno16605", "eno16615", "eno16625", "eno16905np1", "eno16915np0", "eno16925np1" ], "public": [ "ens4", "eno16895np0" ], "trusted": [ "cni0" ] } }, "all_interface_devices": [ "lo", "eno16495", "eno16505", "eno16595", "eno16605", "eno16615", "eno16625", "eno16895np0", "eno16905np1", "eno16915np0", "eno16925np1", "tap0", "kube-ipvs0", "flannel.1", "cni0", "veth4ed8314a", "vethdd87277f", "vetha654be26", "veth4965932b", "vethf367a483", "veth7de8e7b4", "veth70a8cbe4", "veth100d6b8c", "vethf6e6d761", "vethc5ec0f56", "vethccc124f9", "veth7e8b178c", "vethf03364a0", "veth45501887", "veth18a348c0", "vethff692652", "veth6f91fb46", "veth7f0e0c86", "veth4e7e3465", "veth9615b156", "veth1289172a", "veth7c321718", "veth4edade21", "vethd3b6d7b1", "veth0a2d4590", "veth9164e3b2", "vethc7292293", "veth8b7d1132", "vethcc03bd08", "veth41c49f31", "veth3ca934a4", "veth05543e86", "veth038616fb", "veth66452778", "vethd14607aa", "veth6adfac1f", "vethf4407bc9", "veth2717eee6", "veth1f358ccf", "veth020ee1de", "vethf09d7527", "vethc7ed295a", "vethdf6863cf", "vethe9ff14ba", "vethd62a11d4", "veth83018280", "vethc7a04667", "vethcdc6ec2e", "vethae10f1e3", "vethddd00fcf", "veth00181e0a", "veth30e0eaf8", "veth015ed3c5", "veth015d5441", "vethd26d575d", "veth07bc4bed", "vethe9147e1f", "veth6d9263ea", "veth3f986a06", "veth949279a0", "veth504de1fc", "veth5b600c2d", "veth22e7c4e3", "veth5fb797f7" ], "vlan_interface_devices": [], "physical_mellanox_devices": [ "eno16495", "eno16505" ], "preferred_interface_devices": { "control": "eth0", "data": "eth1", "license": "eth0" }, "ethernet_interface_devices": [ "eno16495", "eno16505", "eno16595", "eno16605", "eno16615", "eno16625", "eno16895np0", "eno16905np1", "eno16915np0", "eno16925np1" ] }